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1. Feature

    ▶ High Performance

   ▶ High Reliability

   ▶ RoHS Compliant

 2. Electrical Specifications

	Parameter
	Specification
	Remark

	 Pass Band
	DC-800MHz
	

	Insertion Loss 
	≤0.6dB
	

	VSWR 
	≤1.5
	

	Rejection
	≥40dB@1000-2000MHz
	

	Average Power
	500W
	

	Impedance
	50Ω
	


Mechanical Specifications

	Parameter
	Specifications
	Remark

	Dimensions
	240.0 x 80.0 x 40.0 mm

         ( Not including the tuning screws and connectors )
	

	 Connector Type
	 7/16-female
	

	Surface Finish
	Clear Conductive Coating
	


4. Temperature Specifications

	Parameter
	Specifications
	Remark

	Operational Temperature 
	-20 to +70 ℃
	

	Storage Temperature
	-45 to +85 ℃
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